SYMPHONOTE 
6-piece Chamber Symphony Orchestra

Thank you for your interest, and we are pleased to have the opportunity to collaborate with you. This technical rider contains the requirements necessary for the performance to take place under professional conditions and in accordance with the quality standards assumed by the artist. Please forward this document to the technical supplier and ensure that all specifications are fully complied with prior to the event. Compliance with these requirements directly contributes to the success and quality of the artistic production.
1. STAFF 
STAGE PERSONNEL 

· Vocals  					 
· Pan Flute Soloist 					
· Cello
· Violin 1
· Violin 2 
· Viola
· Piano/Keyboards 
· Bass/ Doublebass 

TECHNICAL TEAM
· Sound Engineer
· Sound Technician  
· Driver 

The Organizer shall provide, at its own expense, all equipment and technical services specified in this document, including the sound system, monitoring, backline, lighting, video, LED screens, cabling and related technical infrastructure.
At least 14 days before the event, the Organizer shall provide the Production Manager with all technical information regarding the stage and audio, video and lighting systems for approval prior to contracting the technical suppliers.
During the performance, stage access is restricted exclusively to the artist's team and personnel previously authorized by the Production Manager.
2. STAGE:
Minimum stage dimensions:
Minimum Length: 6m
Minimum Depth: 4m
Platform Height: 0.4 min

The stage and all related structures must comply with all applicable safety and security regulations. If these conditions are not met, the artist reserves the right to cancel the performance.
The Organizer shall ensure optimal temperature conditions in the stage area during soundchecks and the performance. For outdoor events, heating equipment shall be provided during the cold season and fans during the warm season. If the stage temperature falls below 7°C, a minimum of 5 industrial heaters rated at a minimum of 15 kW each shall be provided.
3. SOUND
A high-performance professional P.A. system, appropriately sized for the venue (indoor/outdoor), capable of providing uniform coverage and adequate sound pressure throughout the entire audience area. Systems by D&B Audiotechnik, L-Acoustics, Meyer Sound, Martin Audio, EAW, or an equivalent professional system are accepted.
Low-cost audio systems or improvised/DIY constructions are not accepted.
Two shielded S/FTP CAT5e/CAT6/CAT7 lines shall be provided between the stage and the FOH position.
The FOH area must provide a minimum of 1 m of technical space, be centrally positioned in relation to the stage, covered and protected from weather conditions, and comply with all safety regulations.
4. TECHNICAL REQUIREMENTS / BACKLINE 
2 x Microphone Shure ULX-D – Beta58 
1 x straight microphone stand with round base
3 x microphone stands with boom arm
4 x Microphone DPA 4099 Condenser 
3 x DPA VIOLIN CLIP 
1 X DPA CELLO CLIP 
2 x DI Stereo Radial / Klark Teknik 
10 x cables XLR
3 x Cables Jack  
8 x Music Stands 
4 x power supplies 230V / 16A 

The electrical supply must be stable at 230V. In the event of voltage fluctuations, the artist reserves the right not to use the equipment until the issue has been resolved.
5. MONITORING
One stereo In-Ear system, preferably Shure PSM 900 or a professional equivalent, as well as 4 stage monitors (wedges), preferably L-Acoustics X15 or D&B Audiotechnik M4, shall be provided.
6. VIDEO
1 x LED screen with minimum dimensions of 6 m x 3 m 
All LED panels must be from the same production series
1 x VJ available for the entire duration of the show. 

7. LIGHTING
1 x lighting operator available for the entire duration of the show
6 x Moving Head Spot 
6 x Moving Head Wash 

Once installed, the backline may not be moved or removed from the stage. 
Backline-ul este destinat exclusiv utilizării de către echipa Symphonoteși nu poate fi folosit împreună cu alți artiști.
The Organizer shall provide storage space for the equipment and ensure that the entire technical infrastructure is ready before the team's arrival.
8. LOAD IN / SETUP / SOUNDCHECK / LOAD OUT
Load In: 30 min
Setup: 30 min
Soundcheck: 30 min
Load Out: 30 min

In the event of technical issues beyond the artist's team's control, we reserve the right to adjust the schedule in order to conduct the soundcheck under optimal conditions.
If any requirements in this rider cannot be fully met, the Organizer is requested to contact the technical department in advance to identify alternative solutions.
The lighting operator, sound engineer and stage manager must be present throughout the entire setup and soundcheck.
9. SCHEDULE
The final schedule for the performance day (setup, soundchecks, stage changes and access times) shall be mutually agreed upon and communicated prior to the event.
10. LOCAL TECHNICAL TEAM
The Organizer shall provide qualified technical personnel for sound, lighting and video, present throughout setup, soundchecks and the performance. The technical team must be at the stage at least one hour before the start of soundchecks and ensure that all equipment is fully operational.
Contact:
Neamtu Constantin – 0762276387 (Sound Engineer) 
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10-piece Chamber Symphony Orchestra

Thank you for your interest, and we are pleased to have the opportunity to collaborate with you. This technical rider contains the requirements necessary for the performance to take place under professional conditions and in accordance with the quality standards assumed by the artist. Please forward this document to the technical supplier and ensure that all specifications are fully complied with prior to the event. Compliance with these requirements directly contributes to the success and quality of the artistic production.
11. STAFF 
STAGE PERSONNEL 

· Vocals  					 
· Pan Flute Soloist
· 6 Violins 					
· Cello
· Viola
· Keyboards 
· Bass 

TECHNICAL TEAM
· Sound Engineer
· Sound Technician  
· Driver 

The Organizer shall provide, at its own expense, all equipment and technical services specified in this document, including the sound system, monitoring, backline, lighting, video, LED screens, cabling and related technical infrastructure.
At least 14 days before the event, the Organizer shall provide the Production Manager with all technical information regarding the stage and audio, video and lighting systems for approval prior to contracting the technical suppliers.
During the performance, stage access is restricted exclusively to the artist's team and personnel previously authorized by the Production Manager.
12. STAGE:
Minimum stage dimensions:
Minimum Length: 6m
Minimum Depth: 4m
Platform Height: 0.4  min

The stage and all related structures must comply with all applicable safety and security regulations. If these conditions are not met, the artist reserves the right to cancel the performance.
The Organizer shall ensure optimal temperature conditions in the stage area during soundchecks and the performance. For outdoor events, heating equipment shall be provided during the cold season and fans during the warm season. If the stage temperature falls below 7°C, a minimum of 5 industrial heaters rated at a minimum of 15 kW each shall be provided.
13. SOUND
A high-performance professional P.A. system, appropriately sized for the venue (indoor/outdoor), capable of providing uniform coverage and adequate sound pressure throughout the entire audience area. Systems by D&B Audiotechnik, L-Acoustics, Meyer Sound, Martin Audio, EAW, or an equivalent professional system are accepted.
Low-cost audio systems or improvised/DIY constructions are not accepted.
Two shielded S/FTP CAT5e/CAT6/CAT7 lines shall be provided between the stage and the FOH position.
The FOH area must provide a minimum of 1 m of technical space, be centrally positioned in relation to the stage, covered and protected from weather conditions, and comply with all safety regulations.
14. TECHNICAL REQUIREMENTS / BACKLINE 
2 x Microphone Shure ULX-D – Beta58 
1 x straight microphone stand with round base
3 x microphone stands with boom arm
8 x Microphone DPA 4099 Condenser 
7 x DPA VIOLIN CLIP 
1 X DPA CELLO CLIP 
2 x DI Stereo Radial / Klark Teknik 
20 x cables XLR
3 x Cables Jack  
12 x Music Stands 
4 x power supplies 230V / 16A 

The electrical supply must be stable at 230V. In the event of voltage fluctuations, the artist reserves the right not to use the equipment until the issue has been resolved.
15. MONITORING
One stereo In-Ear system, preferably Shure PSM 900 or a professional equivalent, as well as 4 stage monitors (wedges), preferably L-Acoustics X15 or D&B Audiotechnik M4, shall be provided.
16. VIDEO
1 x LED screen with minimum dimensions of 6 m x 3 m 
All LED panels must be from the same production series
1 x VJ available for the entire duration of the show. 

17. LIGHTING
1 x lighting operator available for the entire duration of the show
6 x Moving Head Spot 
6 x Moving Head Wash 

Once installed, the backline may not be moved or removed from the stage. 
The backline is intended exclusively for use by the Symphonote team and may not be used by other artists.
The Organizer shall provide storage space for the equipment and ensure that the entire technical infrastructure is ready before the team's arrival.
18. LOAD IN / SETUP / SOUNDCHECK / LOAD OUT
Load In: 30 min
Setup: 30 min
Soundcheck: 60 min
Load Out: 30 min

In the event of technical issues beyond the artist's team's control, we reserve the right to adjust the schedule in order to conduct the soundcheck under optimal conditions.
If any requirements in this rider cannot be fully met, the Organizer is requested to contact the technical department in advance to identify alternative solutions.
The lighting operator, sound engineer and stage manager must be present throughout the entire setup and soundcheck.
19. SCHEDULE
The final schedule for the performance day (setup, soundchecks, stage changes and access times) shall be mutually agreed upon and communicated prior to the event.
20. LOCAL TECHNICAL TEAM
The Organizer shall provide qualified technical personnel for sound, lighting and video, present throughout setup, soundchecks and the performance. The technical team must be at the stage at least one hour before the start of soundchecks and ensure that all equipment is fully operational.
Contact:
Neamtu Constantin – 0762276387 (Sound Engineer) 
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18-piece Symphony Orchestra
Thank you for your interest, and we are pleased to have the opportunity to collaborate with you. This technical rider contains the requirements necessary for the performance to take place under professional conditions and in accordance with the quality standards assumed by the artist. Please forward this document to the technical supplier and ensure that all specifications are fully complied with prior to the event. Compliance with these requirements directly contributes to the success and quality of the artistic production.
21. STAFF 
STAGE PERSONNEL 

· Vocals  					 
· Pan Flute Soloist
· 10 Violins					
· 2 Cellos
· 2 Violas
· Keyboards/Piano
· Bass / Doublebass
· Drums

TECHNICAL TEAM
· Sound Engineer
· Sound Technician  
· Driver 

The Organizer shall provide, at its own expense, all equipment and technical services specified in this document, including the sound system, monitoring, backline, lighting, video, LED screens, cabling and related technical infrastructure.
At least 14 days before the event, the Organizer shall provide the Production Manager with all technical information regarding the stage and audio, video and lighting systems for approval prior to contracting the technical suppliers.
During the performance, stage access is restricted exclusively to the artist's team and personnel previously authorized by the Production Manager.
22. STAGE:
Minimum stage dimensions:
Minimum Length: 8 m
Minimum Depth: 5 m
Platform Height: 0.4  min

The stage and all related structures must comply with all applicable safety and security regulations. If these conditions are not met, the artist reserves the right to cancel the performance.
The Organizer shall ensure optimal temperature conditions in the stage area during soundchecks and the performance. For outdoor events, heating equipment shall be provided during the cold season and fans during the warm season. If the stage temperature falls below 7°C, a minimum of 5 industrial heaters rated at a minimum of 15 kW each shall be provided.
23. SOUND
A high-performance professional P.A. system, appropriately sized for the venue (indoor/outdoor), capable of providing uniform coverage and adequate sound pressure throughout the entire audience area. Systems by D&B Audiotechnik, L-Acoustics, Meyer Sound, Martin Audio, EAW, or an equivalent professional system are accepted.
Low-cost audio systems or improvised/DIY constructions are not accepted.
Two shielded S/FTP CAT5e/CAT6/CAT7 lines shall be provided between the stage and the FOH position.
The FOH area must provide a minimum of 2 m of technical space, be centrally positioned in relation to the stage, covered and protected from weather conditions, and comply with all safety regulations.
24. TECHNICAL REQUIREMENTS / BACKLINE 
2 x Microphone Shure ULX-D – Beta58 
1 x straight microphone stand with round base
6 x microphone stands with boom arm
15 x Microphone DPA 4099 Condenser 
12 x DPA VIOLIN CLIP 
2 X DPA CELLO CLIP
1 X DPA Double Bass CLIP  
3 x DI Stereo Radial / Klark Teknik 
40 x cables XLR
4 x Cables Jack  
15 x Music Stands 
4 x power supplies 230V / 16A 
Drum Microphone Set

The electrical supply must be stable at 230V. In the event of voltage fluctuations, the artist reserves the right not to use the equipment until the issue has been resolved.
25. MONITORING
The following shall be provided: 
· 2 stereo In-Ear systems, preferabil Shure PSM 900 or equivalent.
· 7 stage monitors (wedge) L-Acoustics X15 or D&B Audiotechnik M4.

26. VIDEO
1 x LED screen with minimum dimensions of 6 m x 3 m 
All LED panels must be from the same production series
1 x VJ available for the entire duration of the show. 

27. LIGHTING
1 x lighting operator available for the entire duration of the show
6 x Moving Head Spot 
6 x Moving Head Beam 
6 x Moving Head Wash 
4 X Fresnel 
2 X Blinder 

Once installed, the backline may not be moved or removed from the stage.
The backline is intended exclusively for use by the Symphonote team and may not be used by other artists.
The Organizer shall provide storage space for the equipment and ensure that the entire technical infrastructure is ready before the team's arrival.
28. LOAD IN / SETUP / SOUNDCHECK / LOAD OUT
Load In: 30 min
Setup: 60 min
Soundcheck: 60 min
Load Out: 30 min

In the event of technical issues beyond the artist's team's control, we reserve the right to adjust the schedule in order to conduct the soundcheck under optimal conditions.
If any requirements in this rider cannot be fully met, the Organizer is requested to contact the technical department in advance to identify alternative solutions.
The lighting operator, sound engineer and stage manager must be present throughout the entire setup and soundcheck.
29. SCHEDULE
The final schedule for the performance day (setup, soundchecks, stage changes and access times) shall be mutually agreed upon and communicated prior to the event.
30. LOCAL TECHNICAL TEAM
The Organizer shall provide qualified technical personnel for sound, lighting and video, present throughout setup, soundchecks and the performance. The technical team must be at the stage at least one hour before the start of soundchecks and ensure that all equipment is fully operational.
Contact:
Neamtu Constantin – 0762276387 (Sound Engineer) 
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24-piece Symphony Orchestra
Thank you for your interest, and we are pleased to have the opportunity to collaborate with you. This technical rider contains the requirements necessary for the performance to take place under professional conditions and in accordance with the quality standards assumed by the artist. Please forward this document to the technical supplier and ensure that all specifications are fully complied with prior to the event. Compliance with these requirements directly contributes to the success and quality of the artistic production.
31. STAFF 
STAGE PERSONNEL 

	Vocals  					 
	Piano

	Pan Flute Soloist  			
	Flute

	10 Violins
	Oboe

	2 Violas 
	Clarinet 

	2 Cellos
	French Horn

	Bass / Double Blass
	Trombone

	Drums
	Trumpet

	Keyboards
	




TECHNICAL TEAM
· Sound Engineer
· Sound Technician  
· Driver 

The Organizer shall provide, at its own expense, all equipment and technical services specified in this document, including the sound system, monitoring, backline, lighting, video, LED screens, cabling and related technical infrastructure.
At least 14 days before the event, the Organizer shall provide the Production Manager with all technical information regarding the stage and audio, video and lighting systems for approval prior to contracting the technical suppliers.
During the performance, stage access is restricted exclusively to the artist's team and personnel previously authorized by the Production Manager.
32. STAGE:
Minimum stage dimensions:
Minimum Length: 10 m
Minimum Depth: 7 m
Platform Height: 0.6 min 

The stage and all related structures must comply with all applicable safety and security regulations. If these conditions are not met, the artist reserves the right to cancel the performance.
The Organizer shall ensure optimal temperature conditions in the stage area during soundchecks and the performance. For outdoor events, heating equipment shall be provided during the cold season and fans during the warm season. If the stage temperature falls below 7°C, a minimum of 5 industrial heaters rated at a minimum of 15 kW each shall be provided.
33. SOUND
A high-performance professional P.A. system, appropriately sized for the venue (indoor/outdoor), capable of providing uniform coverage and adequate sound pressure throughout the entire audience area. Systems by D&B Audiotechnik, L-Acoustics, Meyer Sound, Martin Audio, EAW, or an equivalent professional system are accepted.
Low-cost audio systems or improvised/DIY constructions are not accepted.
Two shielded S/FTP CAT5e/CAT6/CAT7 lines shall be provided between the stage and the FOH position.
The FOH area must provide a minimum of 2 m of technical space, be centrally positioned in relation to the stage, covered and protected from weather conditions, and comply with all safety regulations.
34. TECHNICAL REQUIREMENTS / BACKLINE 
2 x Microphone Shure ULX-D – Beta58 
1 x straight microphone stand with round base
12 x microphone stands with boom arm
15 x Microphone DPA 4099 Condenser 
12 x DPA VIOLIN CLIP 
2 X DPA CELLO CLIP
1 X DPA Double Bass CLIP  
3 x DI Stereo Radial / Klark Teknik 
40 x cables XLR
4 x Cables Jack  
15 x Music Stands 
4 x power supplies 230V / 16A 
Drum Microphone Set
6 x Condenser Microphones (Shure KSM137/ SM81) 

The electrical supply must be stable at 230V. In the event of voltage fluctuations, the artist reserves the right not to use the equipment until the issue has been resolved.
35. MONITORING
The following shall be provided:
· 2 stereo In-Ear systems, preferabil Shure PSM 900 or equivalent.
· 7 stage monitors (wedge) L-Acoustics X15 or D&B Audiotechnik M4.

36. VIDEO
1 x LED screen with minimum dimensions of 6 m x 3 m 
All LED panels must be from the same production series
1 x VJ available for the entire duration of the show. 

37. LIGHTING
1 x lighting operator - available for the entire duration of the show
1 x Followspot Operator - available for the entire duration of the show
6 x Moving Head Spot 
6 x Moving Head Beam 
6 x Moving Head Wash
6 X Strobe 
4 X Fresnel 
2 X Blinder 
1 X Followspot 

Once installed, the backline may not be moved or removed from the stage.
The backline is intended exclusively for use by the Symphonote team and may not be used by other artists.
The Organizer shall provide storage space for the equipment and ensure that the entire technical infrastructure is ready before the team's arrival.
38. LOAD IN / SETUP / SOUNDCHECK / LOAD OUT
Load In: 60 min
Setup: 60 min
Soundcheck: 60 min
Load Out: 30 min

In the event of technical issues beyond the artist's team's control, we reserve the right to adjust the schedule in order to conduct the soundcheck under optimal conditions.
If any requirements in this rider cannot be fully met, the Organizer is requested to contact the technical department in advance to identify alternative solutions.
The lighting operator, sound engineer and stage manager must be present throughout the entire setup and soundcheck.
39. SCHEDULE
The final schedule for the performance day (setup, soundchecks, stage changes and access times) shall be mutually agreed upon and communicated prior to the event.
40. LOCAL TECHNICAL TEAM
The Organizer shall provide qualified technical personnel for sound, lighting and video, present throughout setup, soundchecks and the performance. The technical team must be at the stage at least one hour before the start of soundchecks and ensure that all equipment is fully operational.
Contact:
Neamtu Constantin – 0762276387 (Sound Engineer) 
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36-piece Symphony Orchestra
Thank you for your interest, and we are pleased to have the opportunity to collaborate with you. This technical rider contains the requirements necessary for the performance to take place under professional conditions and in accordance with the quality standards assumed by the artist. Please forward this document to the technical supplier and ensure that all specifications are fully complied with prior to the event. Compliance with these requirements directly contributes to the success and quality of the artistic production.
41. STAFF 
STAGE PERSONNEL 

	Vocals			 
	Pian

	Pan Flute Soloist	
	2 Flutes

	14 Violins
	2 Oboes

	4 Violas 
	2 Clarinets 

	3 Cellos
	2 French Horns

	Bass/ Doublebass
	2 Trombones

	Drums
	2 Trumpets

	Keyboards 
	




TECHNICAL TEAM
· Sound Engineer
· Sound Technician  
· Driver 

The Organizer shall provide, at its own expense, all equipment and technical services specified in this document, including the sound system, monitoring, backline, lighting, video, LED screens, cabling and related technical infrastructure.
At least 14 days before the event, the Organizer shall provide the Production Manager with all technical information regarding the stage and audio, video and lighting systems for approval prior to contracting the technical suppliers.
During the performance, stage access is restricted exclusively to the artist's team and personnel previously authorized by the Production Manager.
42. STAGE:
Minimum stage dimensions:
Minimum Length: 12 m
Minimum Depth: 10 m
Platform Height: 1 m min

The stage and all related structures must comply with all applicable safety and security regulations. If these conditions are not met, the artist reserves the right to cancel the performance.
The Organizer shall ensure optimal temperature conditions in the stage area during soundchecks and the performance. For outdoor events, heating equipment shall be provided during the cold season and fans during the warm season. If the stage temperature falls below 7°C, a minimum of 5 industrial heaters rated at a minimum of 15 kW each shall be provided.
43. SOUND
A high-performance professional P.A. system, appropriately sized for the venue (indoor/outdoor), capable of providing uniform coverage and adequate sound pressure throughout the entire audience area. Systems by D&B Audiotechnik, L-Acoustics, Meyer Sound, Martin Audio, EAW, or an equivalent professional system are accepted.
Low-cost audio systems or improvised/DIY constructions are not accepted.
Two shielded S/FTP CAT5e/CAT6/CAT7 lines shall be provided between the stage and the FOH position.
The FOH area must provide a minimum of 2 m of technical space, be centrally positioned in relation to the stage, covered and protected from weather conditions, and comply with all safety regulations.
44. TECHNICAL REQUIREMENTS / BACKLINE 
2 x Microphone Shure ULX-D – Beta58 
1 x straight microphone stand with round base
12 x microphone stands with boom arm
22 x Microphone DPA 4099 Condenser 
18 x DPA VIOLIN CLIP 
3 X DPA CELLO CLIP
1 X DPA Double Bass CLIP  
3 x DI Stereo Radial / Klark Teknik 
50 x cables XLR
4 x Cables Jack  
15 x Music Stands 
6 x power supplies 230V / 16A 
Drum Microphone Set
12 x Condenser Microphones (Shure KSM137/ SM81) 

The electrical supply must be stable at 230V. In the event of voltage fluctuations, the artist reserves the right not to use the equipment until the issue has been resolved.
45. MONITORING
The following shall be provided: 
· 2 stereo In-Ear systems, preferabil Shure PSM 900 or equivalent
· 7 stage monitors (wedge) L-Acoustics X15 or D&B Audiotechnik M4.

46. VIDEO
1 x LED screen with minimum dimensions of 8 m x 3 m 
All LED panels must be from the same production series
1 x VJ available for the entire duration of the show. 

47. LIGHTING
1 x lighting operator - available for the entire duration of the show
1 x Followspot Operator - available for the entire duration of the show
6 x Moving Head Spot 
6 x Moving Head Beam 
6 x Moving Head Wash
6 X Strobe 
4 X Fresnel 
2 X Blinder 
1 X Followspot 

Once installed, the backline may not be moved or removed from the stage.
The backline is intended exclusively for use by the Symphonote team and may not be used by other artists.
The Organizer shall provide storage space for the equipment and ensure that the entire technical infrastructure is ready before the team's arrival.
48. LOAD IN / SETUP / SOUNDCHECK / LOAD OUT
Load In: 60 min
Setup: 90 min
Soundcheck: 60 min
Load Out: 30 min

In the event of technical issues beyond the artist's team's control, we reserve the right to adjust the schedule in order to conduct the soundcheck under optimal conditions.
If any requirements in this rider cannot be fully met, the Organizer is requested to contact the technical department in advance to identify alternative solutions.
The lighting operator, sound engineer and stage manager must be present throughout the entire setup and soundcheck.
49. SCHEDULE
The final schedule for the performance day (setup, soundchecks, stage changes and access times) shall be mutually agreed upon and communicated prior to the event.
50. LOCAL TECHNICAL TEAM
The Organizer shall provide qualified technical personnel for sound, lighting and video, present throughout setup, soundchecks and the performance. The technical team must be at the stage at least one hour before the start of soundchecks and ensure that all equipment is fully operational.
Contact:
Neamtu Constantin – 0762276387 (Sound Engineer) 
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